

***ACC Clear™* Anti-Fog Coatings**

**Anti-Fog Coatings for Injection molding**

***ACC Clear****™* injection molded coatings provide instant, long lasting Anti-Fog protection for unsurpassed product clarity. ***ACC Clear****™* injection molded coatings are water-based formulations, which can be spray applied directly to formed parts post forming. Our ***ACC Clear****™* technology also features slip, mold-release and de-nesting properties necessary for efficient processing.

***ACC Clear****™* Anti-Fog coatings are supplied in either 440lbs drums or 2200lb totes for easy handling and storage.

PRODUCT FEATURES:

Versatile: *ACC Clear™* Anti–Fog coatings provide instant, long lasting anti-fog protection for a variety of Hot & Cold Fill/Storage applications. *ACC Clear™* coatings deliver proven anti-fog properties for wide array of rigid substrates including APET, RPET, PP, OPS, HIPS, PLA and many others.

Sealable: *ACC Clear™* Anti-Fog coatings can be designed with seal-through technology, which allows formed parts to be used in conjunction with lidding films and labeling stock.

FDA Compliant: *ACC Clear™* Anti–Fog coatings offer full FDA compliance for direct food contact and under food additive regulations.

Methods: *ACC Clear™* Anti-Fog coatings can be applied via Spray coating equipment. Our *ACC Clear™* coatings can be also modified around existing coating equipment.

*Please contact your ACC Coatings representative for further information and detailed product recommendations for your application.*